[config]
; Kernel number from kernel list section to be loaded by default
default=1

; Waiting time (in seconds) after which kernel mentioned in "default"
; will be loaded
timeout=15

; Debug options
;dbflags=0x11
dbflags=0

; Debug port
; com port address
; no debug output if statment is omited (but log still accessible 
; through copy from oemhlp$ - see below)
;dbport=0
;dbport=0x3f8
;dbport=0xEC00

; Enable Ctrl-C check for kernel debugger. This is optional for kernels
; beginning from revision 2970. Older kernels always have this check enabled.
; This option ignored if no debug port specified.
; Ctrl-C check allows KDB popup when Ctrl-C is passed via serial link but
; adds two problems:
; - frequent serial port reads cause overall performance degradation
; - the serial port can't be used for something else except KDB because these
;   reads destroy data which are received by the port
;ctrlc=1

; You have full COM port link cable (with hardware flow control support)
;fullcable=1

; Show PC memory table as it reported by BIOS, do nothing if absent
; or defined as 0.
; Warning: this option will make PAUSE on boot!
;showmem=1

; Hide from OS/2 one of memory blocks from list above.
; Block specified by start address (>1Mb, block at 1Mb required for OS/2
; boot). 
; You can add up to five such keys into [config] section.
; note: OS2LDR ignore too small blocks (<64k) by itself.
;removemem=0x20000000

; Color values for the startup menu
; byte 0 - text color
; byte 1 - color of selected row
; byte 2 - background color
; byte 3 - border color
; defauls are:
;menupalette=0x0F070F01

; Show b/w tty style menu with ugly kernel selection by numeric key ;)
; It use BIOS text output only, so suitable for some strange reasons.
;ttymenu = 1 

; Reset video mode to default 80x25, before menu output (fix for some
; strange BIOS bugs too)
;resetmode=1

; OS/4 kernel only (rev>=2075)
; Turn on memory files. Kernel will preload all files, located in:
; - BASEDEV and PSD statements of config.sys
; - os4krnl.ini
; - snoop.lst
; - and predefined list of files: PREVIOUS.DAT, ISAPNP.SYS, ISAPNP.SNP, 
;   RESOURCE.SYS, CLOCK01.SYS, SCREEN01.SYS, KBDBASE.SYS, SNOOP.LST,
;   PNP.SYS, ACPI.CFG, IBMKBD.SNP, PCIBUS.SNP, PREVIOUS.ACP, PCIDEV.TBL
;
preload = 1

; set log size for debug to X kilobytes.
; The value will rounded down to nearest 64k border, but not lower 64k.
; This key can be added to config session (for all kernels)
; Boot log avalable by copying it to file:
;   "copy kernlog$ my.log"
LOGSIZE=128

; Set VIRTUALADDRESSLIMIT for OS/4 kernel
VALIMIT = 3072

[kernel]
; Load oryginal os2krnl
os2krnl      =  OS/2 Kernel
; Load os2ldr.ory (oryginal os2ldr) and launch it:
os2ldr.ory   =  Original OS2LDR  ,Restart
; Load os4krnl with config.os4:
os4krnl      =  OS/4 Kernel      ,CFGEXT=os4,LOADSYM
; Examples:
;os2krnl     =  104b_SMP
;os2krnl.dbg =  104b_SMP dbg
;os4krnl     =  OS/4 Debug  Kernel,LOGSIZE=128,PRELOAD,LOADSYM
;os4krnlr    =  OS/4 Retail Kernel,LOGSIZE=128,PRELOAD
;os4krnlr    =  Show driver names,ALTF2
